**DISCRETE WATER PUSH SAMPLER WITH 24” SCREEN**



Push ahead samplers refers to the tool that is driven ahead of the drilling operation, where drilling disturbance has not occurred yet and at a specific depth. After being driven 24’ ahead of the drilling, the device is pulled back a short distance to expose a screen where a bailer can be run in the string to collect a sample.